

Site Readiness Checklist

**Please review items to be completed prior to cabinet delivery and installation.**

1. Any and all existing cabinetry, (if applicable) has been removed. C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png
2. All heating/cooling ductwork is in place as applicable. C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png
3. All plumbing not required has been removed and new rough-in for supply, C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

waste and vent is complete.

1. All electrical not required has been removed and new rough-in for outlets, C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

appliance feeds and cabinet lighting (including both 110v and low voltage)

has been completed.

1. All walls and bulkheads have been drywalled, taped and sanded with primer C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

coat applied at a minimum. Preferably first finish paint coat is done leaving

only touch ups after installation.

1. All trim around doors and windows has been installed. C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png
2. Subfloor and finished flooring has been installed as cabinets are typically installed C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

on finished floors. The exception to this is laminate floating floors which must be

installed around cabinets and islands. Please ensure floor protection is installed prior

to cabinet delivery.

1. Site has power readily available and adequate lighting. C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png
2. Work area to set up tools is heated, indoors and adjacent to installation area C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

for installation and service appointments.

1. Delivery truck (5 ton) and installer can readily access site for the safe C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

delivery of cabinets and loading/unloading of tools. Site must be clear of debris. C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

1. Installation area must be clear of obstructions, heated and allow for cabinets to be

adjacent to the installation area (cannot place in garage).

1. All railings (permanent or temporary) on stairs/openings MUST be installed. C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png
2. Sink and stove cut out templates and specifications are onsite for the installer C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

to cut out or (in the case of solid surface templated tops) for the templater to

take with him for top fabrication.

1. For tile backsplash applications advise the installer of tile thickness to allow C:\Users\apritchard\AppData\Local\Microsoft\Windows\Temporary Internet Files\Content.IE5\2YVXRE3S\50px-Square-symbol.svg[1].png

the light valance to be set accordingly.

1. **If the site is not ready when we deliver and the cabinets need to be returned to our warehouse**

**or if we have to return to put them in the correct room the next day, there will be a *$500 charge* to your account**.

1. If the installation needs to be rescheduled because the site is not ready, we will reschedule on **our next** **best** **available install date**.

I, \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_have read, understand and agree to abide by the above minimum site requirements for delivery and installation.

Signed \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_